Fly.Simvol association and
ROTW, freewares production team for FLY ! II simulator 
http://fly.simvol.org
=================================================
Scenery of COUCHEVEL (LFLJ)

TO BE USED ONLY WITH FLY ! II

by Beralex (ROTW) and Thierry Petris (ROTW)

March 16th, 2005
version: LFLJ_v1
==================================================

------------------
Location
------------------
Scenery of the Courchevel hight altitude airport located in the department of Savoie (France), in the Alps.

-------------------------------
Product description
-------------------------------
Realization:

High detailled scenery with 100% custom models created with BinEdit.


Content:

	LFLJ-readme 				: present file
      Taxi-LFLJ.POD				: files for taxiways LFLJ.TMS and LFLJ.BGR
	Apt-LFLJ.dex 				: creation of AIRPORT.POD file
	Rwy-LFLJ.dex 				: creation of RUNWAY.POD file
	Wpt-LFLJ.dex 				: creation of WAYPOINT.POD file by Azzurro (ROTW)
	scn-LFLJ_v1.POD et scn-LFLJ-v1.scf	: 3D's scenery objects
      LFLJ.MAP et LFLJ.ECW 			: charts
	D004164_sud.POD 				: risess for the TRI version 
	Rotw_mobile_windsocketGv2.pod 	) Windsocket	
	and WindSocketF_v20.dll			) 
						
	You can find VAC chart on this following site "http://www.sia.aviation-civile.gouv.fr/aip/enligne/METROPOLE/AIP/VAC/index.htm#TopOfPage"


------------------
Prerequisite
------------------
To use this scenery it is first necessary to have installed: MaRv2.1.zip (available on fly.simvol.org) to have a dynamic windsocket.

Attention: 
 	- I have included Rotw_mobile_windsocketGv2.pod file if you don't find the MaRv2.1.zip
	- I have also included the previous WindSocketF_v20.dll file if you get some troubles with WindSocketF_v21.dll file included in MaRv2.1.zip


------------------
Installation
------------------

Unzip the contents into a temporary directory.  

A) DEX installation:

1. First, save your AIRPORT.pod, RUNWAY.pod and WAYPOINT.pod files somewhere,
2. Copy the 3 files Apt-LFLJ.dex, Rwy-LFLJ.dex et Wpt-LFLJ.dex in your ...\Fly! II directory,
3. Use DEXIMPORT or DEXIMPORTGUI to import these 3 files.

B) Scenery installation:

1 - Create a "Courchevel" directory in: ...\Fly! II\Scenery,
2 - Place both scn-LFLJ_v1.POD and scn-LFLJ-v1.scf files in this new directory,
3 - Place Taxi-LFLJ.POD file in: ...\Fly! II\Taxiway,
	(you can un-pod the up-dated Fr-Taxiway you have downloaded on Simvol.org then place these 2 files in the data directory and pod again)
4 - Place both LFLJ.MAP and LFLJ.ECW files in: ...\Fly! II\Map,
5 - Place the new D004164_sud.POD file in: ...\Fly! II\Scenery\France SE Elev SRTM to replace the old one,
6 - If you don't have installed the MaRv2.1.zip, place the Rotw_mobile_windsocketGv2.pod file in: ...\Fly! II\Aircraft (or Aircraft \stuff)
	 and the WindSocketF_v20.dll file in ... \Fly! II\Module\pc.


Remarks: 
You can modify the "scenery" option parameters to increase the fluidity (Fps) in regards of high detailled objects, by:
	- decreasing level of details from complex to normal (+ 8/10 fps)
	- decreasing visibility and/or high resolution radius and/or medium resolution radius and/or controlled aircrafts with half values (+ 4/5 fps).
------------------
Thanks
------------------
To Azzurro (ROTW) for his help for Waypoint and maps

-------------------------
Legal notices
-------------------------
Copyright (C) 2005 ROTW

The authors accept no liability concerning the use of this freeware.
TRI is concerned on no account by this addition in its simulator.
This is a freeware and any use or commercial distribution, whatever the means (not free magazine CD-ROM or CD-ROM compilation ...), is strictly forbidden.
Any use of this freeware in other free products requires the ROTW explicit authorization and implies the reproduction, in its entirety, of this file LFLJ-Readme.txt.


Have nice flights!

-------------------------       
Special notices
-------------------------
Homage à Richard

