Fly.Simvol association and
ROTW, freewares production team for FLY ! II simulator 
http://fly.simvol.org
=================================================
Scenery of FAYENCE (LFMF)

TO BE USED ONLY WITH FLY ! II

by Thierry Petris(ROTW)
October 2005
version : LFMF_v1
==================================================

------------------
Location
------------------

	Scenery of Fayence ( LFMF ) in the department of Alpes Maritimes, the french Riviera .
	Soaring area. It's only a day scenery.

-------------------------------
Product description
-------------------------------
Realization:

	High detailled scenery only for Fly!II with 100% custom models created with BinEdit.

Content:

	LFMF-readme.txt				: the present file
      	ALFMF.POD				: files LFMF.TMS et LFMF.BGR for taxyways
	Rwy-LFMF.dex				: update for RUNWAY.POD
	Scn_LFMF_v1.POD and scn-LFMF_v1.scf	: 3D models files
	Modifs_SE.zip				: new textures of grass for the runways		
	MAR_LFMF.POD				: file for LFMF windsocket
	Windsocket_v3c.POD			: file for models of windsockets
	WindSocketF_v30.dll			: Dll for windsockets

You can find the VAC chart on this site "http://www.sia.aviation-civile.gouv.fr/aip/enligne/METROPOLE/AIP/VAC/index.htm#TopOfPage"

------------------
Prerequisite
------------------


------------------
Installation
------------------

Unzip the contents to a temporary directory.  

A) Installation of DEX 

1. Save your RUNWAY.pod files somewhere first,
2. Copy the  file rwy-LFMF.dex in your Fly!II directory,
3. Use DEXIMPORT or DEXIMPORTGUI to import this file,

B) Installation of scenery :

1 - Create a ''Fayence'' directory in : ...\Fly! II\Scenery,
2 - Place both Scn-LFMF_v1.POD and Scn-LFMF_v1.scf files in this directory,
3 - Place ALFMF.POD file in : ...\Fly! II\Taxiway,
	(you can unpod ALFMF file and place these 2 files in the data directory of unpoded Fr-Taxiway you have downloaded on Simvol.org, and pod again all the files)

C) Installation of new textures:

1 - unpod the file Cannes_v13.POD in a temporary directory, (I use DRAGPODER from Roland)
2 - unpod the file Modifs_SE.zip also in another temporary directory,
3 - copy all the unpoded files from the temporary repertory of Modifs_SE.zip in the temporary directory  ...../DATA/D004162 of Cannes_v13.POD,
4 - pod the temporary directory Cannes_v13.POD in Cannes_v13R.POD et think to modify the file Visicannesscene.scf 
		<file> ---- pod file ----
		Cannes_v13R.pod


D) Installation for windsocket :

1 - Place both MAR_LFMF.POD et Windsocket_v3c.POD files in ...\Fly! II\Aircraft\MaR (or stuff or the name you want), éventualy create it.
2 - Place WindSocketF_v30.dll file in : ...\Fly! II\Module\PC
	Remarks : if you already installed MaRv3 (available on fly.simvol.org) you only have to put the
			MAR_LFMF.POD file in ....\Fly! II\Aircraft\MaR (or stuff or ...) 



Remarks : you can increase or decrease the fluidity by modifying the levels of the environnement menu.
		The fluidity can decrease when arriving from west if you have the two following sceneries
		already installed : Cannes-Mandelieu (LFMD) and Nice-Cote d'Azur (LFMN).

------------------
Thanks
------------------
Beralex and TJ, both from ROTW, for their helps

-------------------------
Legal notices
-------------------------
Copyright (C) 2005 ROTW

The author accepts no liability concerning the use of this freeware.
TRI is concerned on no account by this addition in its simulator.
This is a freeware and any use or commercial distribution, whatever the means (not free magazine CD-ROM or CD-ROM compilation ...), is strictly forbidden.
Any use of this freeware in other free products requires the ROTW explicit authorization and implies the reproduction, in its entirety, of this file LFLG-readme.txt.


Have nice flights!

-------------------------       
Special notices
-------------------------
Homage to Richard
