Fly.Simvol association and
ROTW, freewares production team for FLY ! II simulator 
http://fly.simvol.org
=================================================
Scenery of LA MOLE - Saint-Tropez (LFTZ)

TO BE USED ONLY WITH FLY ! II

by Thierry Petris (ROTW)

May 24 th, 2005
version: LFTZ_v1
==================================================

------------------
Location
------------------
Scenery of the La Môle Saint-Tropez airport located in the department of Var on French Riviera (France).

-------------------------------
Product description
-------------------------------
Realization:

High detailled scenery with 100% custom models created with BinEdit.


Content:

	LFTZ-readme 				: present file
    	ALFTZ.POD				: files for taxiways LFLJ.TMS and LFLJ.BGR
	Scn_LFTZ_v1.POD & scn-LFTZ_v1.scf	: 3D's scenery objects
	Rwy-Lftz.dex				: update for RUNWAY.POD
  	MaR_4161v1.POD & mar-4161v1.scf	)
	Rotw_mobile_windsocketGv2.pod 		) Windsocket	
	and WindSocketF_v20.dll			) 
						
	You can find VAC chart on this following site "http://www.sia.aviation-civile.gouv.fr/aip/enligne/METROPOLE/AIP/VAC/index.htm#TopOfPage"


------------------
Prerequisite
------------------
To use this scenery it is first necessary to have installed: MaRv2.1.zip (available on fly.simvol.org) to have a dynamic windsocket.

Attention: 
 	- I have included Rotw_mobile_windsocketGv2.pod file if you don't find the MaRv2.1.zip
	- I have also included the previous WindSocketF_v20.dll file if you get some troubles with WindSocketF_v21.dll file included in MaRv2.1.zip
	- The windsocket will not be dynamic, but only static, if you have installed the Gap 3D scenery (LFNA): Tallardv3. You have to desactivate
		the LFNAv3.scf file

------------------
Installation
------------------

Unzip the contents into a temporary directory.  

A) Installation of DEX 

1. Save your RUNWAY.pod files somewhere first,
2. Copy the Rwy-Lftz.dex files in your Fly!II directory, or where you have your DexImport tool,
3. Use DEXIMPORT or DEXIMPORTGUI to import these file,

B) Scenery installation:


1 - Create a "La Mole" directory in: ...\Fly! II\Scener,
2 - Place both Scn_LFTZ_v1.POD & scn-LFTZ_v1.scf files in this new directory,

3 - Place both MaR_4161v1.POD & mar-4161v1.scf files also in this new directory,

4 - Place ALFTZ.POD file in: ...\Fly! II\Taxiway,
	(you can un-pod the up-dated Fr-Taxiway you have downloaded on Simvol.org then place these 2 files in the data directory and pod again)

6 - If you don't have installed the MaRv2.1.zip, place the Rotw_mobile_windsocketGv2.pod file in: ...\Fly! II\Aircraft (or Aircraft \stuff)
	 and the WindSocketF_v20.dll file in ... \Fly! II\Module\pc.


Remarks: 
You can modify the "scenery" option parameters to increase the fluidity (Fps) in regards of high detailled objects, by:
	- decreasing level of details from complex to normal (+ 8/10 fps)
	- decreasing visibility and/or high resolution radius and/or medium resolution radius and/or controlled aircrafts with half values (+ 4/5 fps).
------------------
Thanks
------------------
To Azzurro for his dex.

-------------------------
Legal notices
-------------------------
Copyright (C) 2005 ROTW

The authors accept no liability concerning the use of this freeware.
TRI is concerned on no account by this addition in its simulator.
This is a freeware and any use or commercial distribution, whatever the means (not free magazine CD-ROM or CD-ROM compilation ...), is strictly forbidden.
Any use of this freeware in other free products requires the ROTW explicit authorization and implies the reproduction, in its entirety, of this file LFLJ-Readme.txt.


Have nice flights and enjoy the French Riviera!

-------------------------       
Special notices
-------------------------
Homage to Richard

